# Ender-3 V3 SE Firmware with Linear Advance

## Changelog:
1. Activated Linear Advance (default K 0.045)
2. 300°C max nozzle temperature (from 260)
3. Rised limit for bed from 100°C to 110°C
4. Changed Z max speed from 10 to 30
